# RUN: llc -mcpu=gfx900 -march=amdgcn -verify-machineinstrs -run-pass post-RA-hazard-rec %s -o - | FileCheck %s

# If an INLINEASM statement is preceded by a vmem store of more than 8 bytes *and*
# the INLINEASM defs the vregs holding the data-to-be-stored by that preceding store,
# then the hazard recognizer should insert a s_nop in between them.

...

# GCN-LABEL: name: hazard-inlineasm
# CHECK: FLAT_STORE_DWORDX4
# CHECK-NEXT: S_NOP 0
# CHECK-NEXT: INLINEASM

---
name: hazard-inlineasm

body: |
  bb.0:
   FLAT_STORE_DWORDX4 $vgpr49_vgpr50, $vgpr26_vgpr27_vgpr28_vgpr29, 0, 0, 0, implicit $exec, implicit $flat_scr
   INLINEASM &"v_mad_u64_u32 $0, $1, $2, $3, $4", 0, 2621450, def $vgpr26_vgpr27, 2818058, def dead $sgpr14_sgpr15, 589833, $sgpr12, 327689, killed $vgpr51, 2621449, $vgpr46_vgpr47
   S_ENDPGM
...


