Request: VGATHERDPS DISP_WIDTH:8, MEM_WIDTH:64, MEM0:zmmword ptr [RBP+ZMM0*8], MODE:2, REG0:ZMM9, REG1:K7, SMODE:2
OPERAND ORDER: REG0 REG1 MEM0 
Encodable! 62727D4F924CC500
.byte 0x62,0x72,0x7d,0x4f,0x92,0x4c,0xc5,0x00
