Attempting to decode: 48 0f 07 
iclass SYSRET	category SYSRET	ISA-extension LONGMODE	ISA-set LONGMODE
instruction-length 3
operand-width 64
effective-operand-width 64
effective-address-width 64
stack-address-width 64
iform-enum-name SYSRET
iform-enum-name-dispatch (zero based) 0
iclass-max-iform-dispatch 1
Operands
#   TYPE               DETAILS        VIS  RW       OC2 BITS BYTES NELEM ELEMSZ   ELEMTYPE   REGCLASS
#   ====               =======        ===  ==       === ==== ===== ===== ======   ========   ========
0   REG0              REG0=RIP SUPPRESSED   W         Q   64     8     1     64        INT         IP
1   REG1           REG1=RFLAGS SUPPRESSED   W         Y   64     8     1     64        INT      FLAGS
Memory Operands
  MemopBytes = 0
FLAGS:
  must-write-rflags id-mod vip-mod vif-mod ac-mod rf-0 nt-mod iopl-mod of-mod df-mod if-mod tf-mod sf-mod zf-mod af-mod pf-mod cf-mod 
       read:                                mask=0x0
    written: of sf zf af pf cf df vif iopl if ac rf nt tf id vip  mask=0x3d7fd5
  undefined:                                mask=0x0
ATTRIBUTES: NOTSX PROTECTED_MODE RING0 
RING0 only
Number of legacy prefixes: 1 
ISA SET: [LONGMODE]
0	CPUID BIT NAME: [INTEL64]
	Leaf 0x80000001, subleaf 0x00000000, EDX[29]
