Setting chip to PENRYN_E
Attempting to decode: 0f 01 d0 
iclass XGETBV	category XSAVE	ISA-extension XSAVE	ISA-set XSAVE
instruction-length 3
operand-width 32
effective-operand-width 32
effective-address-width 32
stack-address-width 32
iform-enum-name XGETBV
iform-enum-name-dispatch (zero based) 0
iclass-max-iform-dispatch 1
Operands
#   TYPE               DETAILS        VIS  RW       OC2 BITS BYTES NELEM ELEMSZ   ELEMTYPE   REGCLASS
#   ====               =======        ===  ==       === ==== ===== ===== ======   ========   ========
0   REG0              REG0=ECX SUPPRESSED   R         D   32     4     1     32        INT        GPR
1   REG1              REG1=EDX SUPPRESSED   W         D   32     4     1     32        INT        GPR
2   REG2              REG2=EAX SUPPRESSED   W         D   32     4     1     32        INT        GPR
3   REG3             REG3=XCR0 SUPPRESSED   R         Q   64     8     1     64        INT        XCR
Memory Operands
  MemopBytes = 0
ATTRIBUTES: 
ISA SET: [XSAVE]
0	CPUID BIT NAME: [XSAVE]
	Leaf 0x00000001, subleaf 0x00000000, ECX[26]
1	CPUID BIT NAME: [OSXSAVE]
	Leaf 0x00000001, subleaf 0x00000000, ECX[27]
