Request: VSCATTERPF0DPS DISP_WIDTH:8, MEM_WIDTH:1, MEM0:byte ptr [RAX+ZMM0*1-0x1], MODE:2, REG0:K0, SMODE:2
OPERAND ORDER: MEM0 REG0 
Could not encode: VSCATTERPF0DPS MEM1:RAX,ZMM0,1,ff k0 
Error code was: GENERAL_ERROR
[XED CLIENT ERROR] Dying
