Attempting to decode: 00 00 
iclass ADD	category BINARY	ISA-extension BASE	ISA-set I86
instruction-length 2
operand-width 8
effective-operand-width 32
effective-address-width 32
stack-address-width 32
iform-enum-name ADD_MEMb_GPR8
iform-enum-name-dispatch (zero based) 11
iclass-max-iform-dispatch 18
Operands
#   TYPE               DETAILS        VIS  RW       OC2 BITS BYTES NELEM ELEMSZ   ELEMTYPE   REGCLASS
#   ====               =======        ===  ==       === ==== ===== ===== ======   ========   ========
0   MEM0           (see below)   EXPLICIT  RW         B    8     1     1      8       UINT    INVALID
1   REG0               REG0=AL   EXPLICIT   R         B    8     1     1      8        INT        GPR
2   REG1           REG1=EFLAGS SUPPRESSED   W         Y   32     4     1     32        INT      FLAGS
Memory Operands
  0    read written SEG= DS BASE= EAX/GPR  ASZ0=32
  MemopBytes = 1
FLAGS:
  must-write-rflags of-mod sf-mod zf-mod af-mod pf-mod cf-mod 
       read:                                mask=0x0
    written:             of sf zf af pf cf  mask=0x8d5
  undefined:                                mask=0x0
ATTRIBUTES: BYTEOP LOCKABLE 
ISA SET: [I86]
