66E811223344
ICLASS: CALL_NEAR   CATEGORY: CALL   EXTENSION: BASE  IFORM: CALL_NEAR_RELBRd   ISA_SET: I86
SHORT: call 0x44332217
Encodable! E811223344
Discrepenacy after re-encoding. dec_len= 6 [66E811223344] enc_olen= 5 [E811223344] for instruction: CALL_NEAR CALL_NEAR_RELBRd BRDISP_WIDTH:32, DF64, DISP_WIDTH:32, EASZ:3, EOSZ:3, LZCNT, MAX_BYTES:6, MEM0:qword ptr [RSP], MEM_WIDTH:8, MODE:2, NOMINAL_OPCODE:232, NPREFIXES:1, P4, POS_DISP:2, POS_NOMINAL_OPCODE:1, PREFIX66, REG0:STACKPUSH, REG1:RIP, RELBR:0x44332211, SMODE:2, TZCNT, USING_DEFAULT_SEGMENT0
0		RELBR/R/D/EXPLICIT/IMM_CONST/1
1		REG0/W/SPW/SUPPRESSED/REG/STACKPUSH
2		REG1/RW/V/SUPPRESSED/NT_LOOKUP_FN/RIP
3		MEM0/W/SPW/SUPPRESSED/IMM_CONST/1
4		BASE0/RW/SSZ/SUPPRESSED/NT_LOOKUP_FN/SRSP
YDIS: call 0x44332217
vs Encode  request: CALL_NEAR BRDISP_WIDTH:32, DF64, DISP_WIDTH:32, EASZ:3, EOSZ:3, LZCNT, MAX_BYTES:6, MEM0:qword ptr [RSP], MEM_WIDTH:8, MODE:2, NOMINAL_OPCODE:232, NPREFIXES:1, P4, POS_DISP:2, POS_NOMINAL_OPCODE:1, PREFIX66, REG0:STACKPUSH, REG1:RIP, RELBR:0x44332211, SMODE:2, TZCNT, USING_DEFAULT_SEGMENT0
OPERAND ORDER: RELBR 

