660F8411223344
ICLASS: JZ   CATEGORY: COND_BR   EXTENSION: BASE  IFORM: JZ_RELBRd   ISA_SET: I86
SHORT: jz 0x44332218
Encodable! 0F8411223344
Discrepenacy after re-encoding. dec_len= 7 [660F8411223344] enc_olen= 6 [0F8411223344] for instruction: JZ JZ_RELBRd BRDISP_WIDTH:32, DF64, DISP_WIDTH:32, EASZ:3, EOSZ:3, LZCNT, MAP:1, MAX_BYTES:7, MODE:2, NOMINAL_OPCODE:132, NPREFIXES:1, OUTREG:RFLAGS, P4, POS_DISP:3, POS_NOMINAL_OPCODE:2, PREFIX66, REG0:RIP, REG1:RFLAGS, RELBR:0x44332211, SMODE:2, SRM:4, TZCNT
0		RELBR/R/D/EXPLICIT/IMM_CONST/1
1		REG0/RW/V/SUPPRESSED/NT_LOOKUP_FN/RIP
2		REG1/R/Y/SUPPRESSED/NT_LOOKUP_FN/RFLAGS
YDIS: jz 0x44332218
vs Encode  request: JZ BRDISP_WIDTH:32, DF64, DISP_WIDTH:32, EASZ:3, EOSZ:3, LZCNT, MAP:1, MAX_BYTES:7, MODE:2, NOMINAL_OPCODE:132, NPREFIXES:1, OUTREG:RFLAGS, P4, POS_DISP:3, POS_NOMINAL_OPCODE:2, PREFIX66, REG0:RIP, REG1:RFLAGS, RELBR:0x44332211, SMODE:2, SRM:4, TZCNT
OPERAND ORDER: RELBR 

