Attempting to decode: 9d 
iclass POPFQ	category POP	ISA-extension LONGMODE	ISA-set LONGMODE
instruction-length 1
operand-width 64
effective-operand-width 64
effective-address-width 64
stack-address-width 64
iform-enum-name POPFQ
iform-enum-name-dispatch (zero based) 0
iclass-max-iform-dispatch 1
Operands
#   TYPE               DETAILS        VIS  RW       OC2 BITS BYTES NELEM ELEMSZ   ELEMTYPE   REGCLASS
#   ====               =======        ===  ==       === ==== ===== ===== ======   ========   ========
0   REG0         REG0=STACKPOP SUPPRESSED   R         Q   64     8     1     64        INT     PSEUDO
1   MEM0           (see below) SUPPRESSED   R         Q   64     8     1     64        INT    INVALID
2  BASE0             BASE0=RSP SUPPRESSED  RW       SSZ   64     8     1     64        INT        GPR
3   REG1           REG1=RFLAGS SUPPRESSED  RW         Y   64     8     1     64        INT      FLAGS
Memory Operands
  0    read BASE= RSP/GPR  ASZ0=64
  MemopBytes = 8
FLAGS:
   reads-rflags id-pop vip-tst vif-mod ac-pop vm-tst rf-0 nt-pop iopl-tst iopl-pop of-pop df-pop if-pop tf-pop sf-pop zf-pop af-pop pf-pop cf-pop 
       read:                   iopl vm vip  mask=0x123000
    written: of sf zf af pf cf df vif iopl if ac rf nt tf id  mask=0x2d7fd5
  undefined:                                mask=0x0
ATTRIBUTES: FIXED_BASE0 NOTSX STACKPOP0 
ISA SET: [LONGMODE]
0	CPUID BIT NAME: [INTEL64]
	Leaf 0x80000001, subleaf 0x00000000, EDX[29]
