Attempting to decode: f2 f3 64 67 3e 66 2e 36 65 26 f3 0f 2c 0f 
iclass CVTTSS2SI	category CONVERT	ISA-extension SSE	ISA-set SSE
instruction-length 14
operand-width 32
effective-operand-width 32
effective-address-width 32
stack-address-width 64
iform-enum-name CVTTSS2SI_GPR32d_MEMss
iform-enum-name-dispatch (zero based) 0
iclass-max-iform-dispatch 4
Operands
#   TYPE               DETAILS        VIS  RW       OC2 BITS BYTES NELEM ELEMSZ   ELEMTYPE   REGCLASS
#   ====               =======        ===  ==       === ==== ===== ===== ======   ========   ========
0   REG0              REG0=ECX   EXPLICIT   W         D   32     4     1     32        INT        GPR
1   MEM0           (see below)   EXPLICIT   R        SS   32     4     1     32     SINGLE    INVALID
Memory Operands
  0    read SEG= GS BASE= EDI/GPR  ASZ0=32
  MemopBytes = 4
ATTRIBUTES: MXCSR SIMD_SCALAR 
F3 PREFIX
67 PREFIX
ANY 66 PREFIX
EXCEPTION TYPE: SSE_TYPE_3
Number of legacy prefixes: 11 
ISA SET: [SSE]
0	CPUID BIT NAME: [SSE]
	Leaf 0x00000001, subleaf 0x00000000, EDX[25]
