Request: VGATHERDPD DISP_WIDTH:8, MEM_WIDTH:64, MEM0:zmmword ptr [RAX+YMM1*1+0x11], MODE:2, REG0:ZMM0, REG1:K7, SMODE:2
OPERAND ORDER: REG0 REG1 MEM0 
Encodable! 62F2FD4F92440811
.byte 0x62,0xf2,0xfd,0x4f,0x92,0x44,0x08,0x11
