Setting chip to SALTWELL
Attempting to decode: 0f 0d 08 
iclass PREFETCHW	category PREFETCH	ISA-extension 3DNOW	ISA-set PREFETCH_NOP
instruction-length 3
operand-width 32
effective-operand-width 32
effective-address-width 32
stack-address-width 32
iform-enum-name PREFETCHW_0F0Dr1
iform-enum-name-dispatch (zero based) 0
iclass-max-iform-dispatch 2
Operands
#   TYPE               DETAILS        VIS  RW       OC2 BITS BYTES NELEM ELEMSZ   ELEMTYPE   REGCLASS
#   ====               =======        ===  ==       === ==== ===== ===== ======   ========   ========
0   MEM0           (see below)   EXPLICIT   R MPREFETCH  512    64     8     64        INT    INVALID
Memory Operands
  0    read SEG= DS BASE= EAX/GPR  ASZ0=32
  MemopBytes = 64
ATTRIBUTES: PREFETCH 
ISA SET: [PREFETCH_NOP]
