Request: MOVSD_XMM EASZ:2, MEM0:dword ptr [EAX], MEM_WIDTH:4, MODE:1, REG0:XMM0, SMODE:1
OPERAND ORDER: REG0 MEM0 
Could not encode: movsd_xmm xmm0 MEM4:eax 
Error code was: GENERAL_ERROR
[XED CLIENT ERROR] Dying
