Attempting to decode: f3 f2 67 66 2e 64 65 36 3e 26 d0 00 
iclass ROL	category ROTATE	ISA-extension BASE	ISA-set I86
instruction-length 12
operand-width 8
effective-operand-width 16
effective-address-width 32
stack-address-width 64
iform-enum-name ROL_MEMb_ONE
iform-enum-name-dispatch (zero based) 8
iclass-max-iform-dispatch 12
Operands
#   TYPE               DETAILS        VIS  RW       OC2 BITS BYTES NELEM ELEMSZ   ELEMTYPE   REGCLASS
#   ====               =======        ===  ==       === ==== ===== ===== ======   ========   ========
0   MEM0           (see below)   EXPLICIT  RW         B    8     1     1      8       UINT    INVALID
1   IMM0               0x1(8b)   IMPLICIT   R         B    8     1     1      8       UINT    INVALID
2   REG0           REG0=RFLAGS SUPPRESSED   W         Y   32     4     1     32        INT      FLAGS
Memory Operands
  0    read written SEG= GS BASE= EAX/GPR  ASZ0=32
  MemopBytes = 1
FLAGS:
  must-write-rflags of-mod cf-mod 
       read:                                mask=0x0
    written:                         of cf  mask=0x801
  undefined:                                mask=0x0
ATTRIBUTES: BYTEOP IMPLICIT_ONE 
F2 PREFIX
67 PREFIX
66-OSZ PREFIX
ANY 66 PREFIX
Number of legacy prefixes: 10 
ISA SET: [I86]
