Attempting to decode: 0f 12 c0 
iclass MOVHLPS	category DATAXFER	ISA-extension SSE	ISA-set SSE
instruction-length 3
operand-width 32
effective-operand-width 32
effective-address-width 32
stack-address-width 32
iform-enum-name MOVHLPS_XMMq_XMMq
iform-enum-name-dispatch (zero based) 0
iclass-max-iform-dispatch 1
Operands
#   TYPE               DETAILS        VIS  RW       OC2 BITS BYTES NELEM ELEMSZ   ELEMTYPE   REGCLASS
#   ====               =======        ===  ==       === ==== ===== ===== ======   ========   ========
0   REG0             REG0=XMM0   EXPLICIT   W         Q   64     8     2     32     SINGLE        XMM
1   REG1             REG1=XMM0   EXPLICIT   R         Q   64     8     2     32     SINGLE        XMM
Memory Operands
  MemopBytes = 0
ATTRIBUTES: 
EXCEPTION TYPE: SSE_TYPE_7
ISA SET: [SSE]
0	CPUID BIT NAME: [SSE]
	Leaf 0x00000001, subleaf 0x00000000, EDX[25]
