660F20C0
ICLASS: MOV_CR   CATEGORY: DATAXFER   EXTENSION: BASE  IFORM: MOV_CR_GPR32_CR   ISA_SET: I86
SHORT: mov eax, cr0
Encodable! 0F20C0
Discrepenacy after re-encoding. dec_len= 4 [660F20C0] enc_olen= 3 [0F20C0] for instruction: MOV_CR MOV_CR_GPR32_CR DF32, EASZ:1, EOSZ:2, HAS_MODRM:2, LZCNT, MAP:1, MAX_BYTES:4, MOD:3, MODRM_BYTE:192, NOMINAL_OPCODE:32, NPREFIXES:1, OUTREG:CR0, P4, POS_MODRM:3, POS_NOMINAL_OPCODE:2, PREFIX66, REG0:EAX, REG1:CR0, SMODE:1, TZCNT
0		REG0/W/D/EXPLICIT/NT_LOOKUP_FN/GPR32_B
1		REG1/R/Y/EXPLICIT/NT_LOOKUP_FN/CR_R
YDIS: mov eax, cr0
vs Encode  request: MOV_CR DF32, EASZ:1, EOSZ:2, HAS_MODRM:2, LZCNT, MAP:1, MAX_BYTES:4, MOD:3, MODRM_BYTE:192, NOMINAL_OPCODE:32, NPREFIXES:1, OUTREG:CR0, P4, POS_MODRM:3, POS_NOMINAL_OPCODE:2, PREFIX66, REG0:EAX, REG1:CR0, SMODE:1, TZCNT
OPERAND ORDER: REG0 REG1 

