Attempting to decode: 9d 
iclass POPFD	category POP	ISA-extension BASE	ISA-set I386
instruction-length 1
operand-width 32
effective-operand-width 32
effective-address-width 32
stack-address-width 32
iform-enum-name POPFD
iform-enum-name-dispatch (zero based) 0
iclass-max-iform-dispatch 1
Operands
#   TYPE               DETAILS        VIS  RW       OC2 BITS BYTES NELEM ELEMSZ   ELEMTYPE   REGCLASS
#   ====               =======        ===  ==       === ==== ===== ===== ======   ========   ========
0   REG0         REG0=STACKPOP SUPPRESSED   R         D   32     4     1     32        INT     PSEUDO
1   MEM0           (see below) SUPPRESSED   R         D   32     4     1     32        INT    INVALID
2  BASE0             BASE0=ESP SUPPRESSED  RW       SSZ   32     4     1     32        INT        GPR
3   REG1           REG1=EFLAGS SUPPRESSED  RW         Y   32     4     1     32        INT      FLAGS
Memory Operands
  0    read SEG= SS BASE= ESP/GPR  ASZ0=32
  MemopBytes = 4
FLAGS:
   reads-rflags id-pop vip-tst vif-mod ac-pop vm-tst rf-0 nt-pop iopl-tst iopl-pop of-pop df-pop if-pop tf-pop sf-pop zf-pop af-pop pf-pop cf-pop 
       read:                   iopl vm vip  mask=0x123000
    written: of sf zf af pf cf df vif iopl if ac rf nt tf id  mask=0x2d7fd5
  undefined:                                mask=0x0
ATTRIBUTES: FIXED_BASE0 NOTSX STACKPOP0 
ISA SET: [I386]
