Attempting to decode: 0f b2 00 00 
iclass LSS	category SEGOP	ISA-extension BASE	ISA-set I386
instruction-length 3
operand-width 32
effective-operand-width 32
effective-address-width 64
stack-address-width 64
iform-enum-name LSS_GPRv_MEMp2
iform-enum-name-dispatch (zero based) 0
iclass-max-iform-dispatch 1
Operands
#   TYPE               DETAILS        VIS  RW       OC2 BITS BYTES NELEM ELEMSZ   ELEMTYPE   REGCLASS
#   ====               =======        ===  ==       === ==== ===== ===== ======   ========   ========
0   REG0              REG0=EAX   EXPLICIT   W         V   32     4     1     32        INT        GPR
1   MEM0           (see below)   EXPLICIT   R        P2   48     6     1     48     STRUCT    INVALID
2   REG1               REG1=SS SUPPRESSED   W         W   16     2     1     16        INT         SR
Memory Operands
  0    read BASE= RAX/GPR  ASZ0=64
  MemopBytes = 6
ATTRIBUTES: NOTSX SCALABLE 
ISA SET: [I386]
